{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工程量清单-发标"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"工程量清单-发标","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"merged":[[0,0,0,8],[16,1,16,6]]}
["ETC改造工程标识标牌制作安装工程-工程量清单"]
["序号","名称","规格","单位","数量","不含税综合单价（元）","含税综合单价\n（元，税率9%）","含税合价\n（元）","备注"]
["一","悬臂式"]
[1,"ETC车道指示标志","2400*3000","座",{"v":2,"d":"2.00"},{"$nulls":3},"ETC 车道指示类标志板（3000*2400*5mm）标志板采用 3mm厚铝合金板制成。标志边缘均采用角铝加固，角铝和滑动槽铝用铆钉铆固在标志板上，铆钉头应打磨平滑。立柱： 351*10*8080，横梁152*10*3900*2  基础：2*2.6*2m，反光膜：底膜IV类，字膜V类"]
["二","单柱式"]
[1,"ETC专用\n保持车距","1100×600+1100×1700","块",{"v":10,"d":"10.00"},{"$nulls":3},"车道岛头标志板，采用公路用玻璃纤维增强塑料等非金属类板材。利用原有杆件，含安装劳务,更换反光膜"]
[2,"ETC/人工\n保持车距","1100×600+1100×1700","块",{"v":2,"d":"2.00"},{"$nulls":3},"车道岛头标志板，采用公路用玻璃纤维增强塑料等非金属类板材。利用原有杆件，含安装劳务，更换反光膜"]
[3,"ETC/人工\n称重","1100×600+1100×1700","块",{"v":2,"d":"2.00"},{"$nulls":3},"车道岛头标志板，采用公路用玻璃纤维增强塑料等非金属类板材。利用原有杆件，含安装劳务，更换反光膜"]
["三","标线"]
[1,"黄色双组分导流防滑标线",null,"㎡",{"$f":"173.32*1","v":173.32},{"$nulls":3},"黄色双组份导流防滑标线；采用热熔反光涂料，并参有玻璃珠，其材料及配比应符合 JT/T 280 的规定。含劳务，按实际计量结算"]
[2,"普通热熔标线",null,"㎡",{"v":396.9,"d":"396.90"},{"$nulls":3},"普通热熔标线，热熔标线厚度为 2mm；采用热熔反光涂料，并参有玻璃珠，其材料及配比应符合 JT/T 280 的规定。含劳务，按实际计量结算"]
[3,"振动热熔标线",null,"㎡",{"v":168,"d":"168.00"},{"$nulls":3},"振动热熔标线底膜的厚度为 1.5mm，凸起部分的厚度为 6mm；采用热熔反光涂料，并参有玻璃珠，其材料及配比应符合 JT/T 280 的规定。含劳务，按实际计量结算"]
[4,"振动热熔车道边缘线",null,"㎡",{"v":173.6,"d":"173.60"},{"$nulls":3},"振动热熔车道边缘线；采用热熔反光涂料，并参有玻璃珠，其材料及配比应符合 JT/T 280 的规定。含劳务，按实际计量结算"]
[5,"热熔文字标线",null,"㎡",{"v":266.4,"d":"266.40"},{"$nulls":3},"热熔文字标线，热熔标线厚度为 2mm；采用热熔反光涂料，并参有玻璃珠，其材料及配比应符合 JT/T 280 的规定。含劳务，按实际计量结算"]
[6,"橡胶警示柱",null,"根",{"v":150,"d":"150.00"}]
[7,"公路反光道钉",null,"个",{"v":150,"d":"150.00"}]
[8,"合计"]